{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["外委"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"外委","index":0,"n_rows":53,"n_cols":7,"rows_kept":53,"merged":[[0,0,0,6],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[3,0,6,0],[3,1,6,1],[3,2,6,2],[3,4,6,4],[3,5,6,5],[3,6,6,6],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,4,8,4],[7,5,8,5],[7,6,8,6],[9,0,10,0],[9,1,10,1],[9,2,10,2],[9,4,10,4],[9,5,10,5],[9,6,10,6],[11,0,12,0],[11,1,12,1],[11,2,12,2],[11,4,12,4],[11,5,12,5],[11,6,12,6],[15,0,24,0],[15,1,24,1],[15,2,24,2],[15,4,24,4],[15,5,24,5],[15,6,24,6],[27,0,29,0],[27,1,29,1],[27,2,29,2],[27,4,29,4],[27,5,29,5],[27,6,29,6],[30,0,33,0],[30,1,33,1],[30,2,33,2],[30,4,33,4],[30,5,33,5],[30,6,33,6],[34,0,35,0],[34,1,35,1],[34,2,35,2],[34,4,35,4],[34,5,35,5],[34,6,35,6],[36,0,38,0],[36,1,38,1],[36,2,38,2],[36,4,38,4],[36,5,38,5],[36,6,38,6],[39,0,46,0],[39,1,46,1],[39,2,46,2],[39,4,46,4],[39,5,46,5],[39,6,46,6],[47,0,52,0],[47,1,52,1],[47,2,52,2],[47,4,52,4],[47,5,52,5],[47,6,52,6],[50,3,51,3]],"flags":["formulas_cached_only"]}
["2025年度春季各系统设备检修项目招标明细"]
["分项","设备编号","项目名称","主要检修内容","不含税报价（元）","增值税专票税率（%）","含税报价（元）"]
[]
[1,null,"工艺管道维修（一）","1.修补窑头沉降室及旁路管道漏点"]
[{"$nulls":3},"2.窑尾收尘器壳体内部漏点修补"]
[{"$nulls":3},"3.窑头收尘器壳体内部漏点修补"]
[{"$nulls":3},"4.原料旋风收尘器工艺管道.漏风修补"]
[2,57.02,"工艺管道维修（二）","1脱硫陶瓷收尘至高温风机进口管道用盲板封堵"]
[{"$nulls":3},"1.预热器4楼部分管道更换（约4米，Φ4000）,安装2个金属膨胀节"]
[3,null,"烧成窑头维修","1.更换回转窑窑头冷风套"]
[{"$nulls":3},"2.更换窑头密封钢片，修复密封底座及下侧灰斗"]
[4,null,"回转窑维修(一)","1、车削轮带、托带轮（三挡）"]
[{"$nulls":3},"2. 三档北托轮工作面挖补、探测。"]
[5,41.05,"立磨维修（一）","1.41.05下料器更换衬板.调整板.转子及壳体侧面修补"]
[6,41.05,"立磨维修（二）","1.更换磨内3#.4#辊护套"]
[7,73.06,"辊盘式煤磨机维修（一）","1.更换11件磨盘瓦.3件辊套"]
[{"$nulls":3},"2.更换拉杆.更换上下关节轴承及下部密封总成"]
[{"$nulls":3},"3.选粉机静叶片检查更换"]
[{"$nulls":3},"4.更换限位板.三脚架找正"]
[{"$nulls":3},"5.补焊喷口环，堆焊磨内壳体磨损部位"]
[{"$nulls":3},"6.检查1.2.3#张紧液压缸及蓄能装置"]
[{"$nulls":3},"7.修复吐渣仓刮料板"]
[{"$nulls":3},"8.修补磨机出口.入口膨胀节.连接管路"]
[{"$nulls":3},"9.下料管修补，磨辊护板更换，限位块更换"]
[{"$nulls":3},"10.检查磨辊轴承，更换轴承密封及耐磨套"]
[8,"73.06P","辊盘式煤磨机维修（二）","1.减速机更换高速轴三件套，检查减速机轴承.推力瓦，更换润滑油"]
[9,65.01,"熟料输送机维修","1. 熟料输送机头尾部链轮.轴承座.机架找正"]
[10,84.31,"1#水泥磨维修","1.筛板改造，共计68块篦板"]
[{"$nulls":3},"2.更换磨进料端衬板第二.第三圈共36块（更换挡料圈共84块)"]
[{"$nulls":3},"3.更换铜夹板2块（长约1.2米，宽约0.1米）"]
[11,84.13,"2#辊压机维修","1.更换动辊（轴承利旧，需将旧辊上的轴承拆下，安装到需更换的辊子上）"]
[{"$nulls":3},"2.西侧壳体焊补"]
[{"$nulls":3},"3.更换4个主液压缸（液压缸拆下后，要外出维修约5天左右才能返厂安装）"]
[{"$nulls":3},"4.更换铜滑道1套（滑道需重新钻孔）"]
[12,84.01,"84.01提升机维修","1.更换提升机上部链轮总成"]
[{"$nulls":3},"2.上托返平找正"]
[13,78.01,"石膏板式喂料机维修","1.更换链条（头尾轮中心距18米）"]
[{"$nulls":3},"2.调换轨道位置（利旧，将两条轨道拆下后左右调换位置安装）"]
[{"$nulls":3},"3.更换头部链轮总成"]
[14,"02.02","矿山锤式破碎机维修","1.破碎机更换转子总成，调节轴承间隙。"]
[{"$nulls":3},"2.检查更换大皮带轮胀套.更换大皮带轮37根窄V带。"]
[{"$nulls":3},"3.拆装破碎机部分壳体，更换机体内部分衬板及螺丝，以及外壳体螺丝，做法兰密封。"]
[{"$nulls":3},"4.更换锤头.锤轴.锤轴挡盖。"]
[{"$nulls":3},"5.补焊壳体磨损位置。"]
[{"$nulls":3},"6.加固破碎机入料口工字钢结构。"]
[{"$nulls":3},"7.加固焊接破碎机下料口.各位置下料溜子以及其他焊接工作。"]
[{"$nulls":3},"8.矿车补焊加固大箱体.大架体.及各开焊处。"]
[15,null,"高压电机反电机厂维修","1.立磨车头滑环维修（含现场拆安）"]
[{"$nulls":3},"2.2#磨辊压机定辊电机（900KW高压10KV）"]
[{"$nulls":3},"3.1#磨辊压机动辊电机（900KW高压10KV）"]
[{"$nulls":3},"4.2#水泥磨主电机（3550KW高压10KV），含现场电机拆卸吊装、维修后电机吊装安装"]
[]
[{"$nulls":3},"5.2#水泥磨排风机电机（800KW高压变频驱动）"]